# westslope_rte

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: Westslope Cutthroat Trout Interagency Conservation Team
      Publication_Date: 5/1/2003
      Title: westslope_rte
      Geospatial_Data_Presentation_Form: vector digital data
      Online_Linkage: \\PC5009\wendi_d_drive\westslope\westslope_rte.shp
  Description:
    Abstract:
      This Latitude-Longitude Identifier (LLID) 1:100,000 hydrography layer edge-matched across state boundaries was used as the primary base-layer for the Westslope Cutthroat Trout Range-wide Assessment. The U.S. Geological Survey (USGS) in Portland, in cooperation with Bonneville Power Administration, the Northwest Power Planning Council, and other Federal and state agencies and NW Indian Tribes produced a 1:100,000-scale River Reach data layer for the Pacific Northwest in the early 1990s. The Pacific Northwest (PNW) River Reach Files are a geo-referenced river reach data layer that encompasses the Columbia River Basin within the conterminous United States, the coasts of Oregon and Washington, Puget Sound in Washington, the Klamath and Goose Lake Basins in southern Oregon and the Bear Lake Basin in southeastern Idaho (PNW Reach File, Gladstone, Oregon: Stream Net, August 2002. <http://www.streamnet.org/pnwr/pnwrhome.html>). River reach files for Montana east of the Continental Divide were obtained from Montana Fish Wildlife and Parks (Streams. Helena, MT: Montana Fish Wildlife and Parks, August 2002 and are available at <http://fwp.state.mt.us/insidefwp/fwplibrary/gis/>). This LLID hydrography layer routes stream segments by uniquely identifying each stream. The polylineM shapefile format allows for increased display speed using ArcView.
    Purpose:
      This hydrography layer was used as the primary base-layer for the Westslope Cutthroat Trout Range-wide Assessment.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 5/1/2003
    Currentness_Reference: publication date
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -121.809257
      East_Bounding_Coordinate: -107.011529
      North_Bounding_Coordinate: 50.555926
      South_Bounding_Coordinate: 42.998269
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus:
        REQUIRED: Reference to a formally registered thesaurus or a similar authoritative source of theme keywords.
      Theme_Keyword: Stream routes
    Place:
      Place_Keyword: Pacific Northwest
  Access_Constraints: Public
  Use_Constraints: Use constrained to analysis at scales of 1:100,000 or smaller.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Wendi Urie
        Contact_Organization: US Forest Service
      Contact_Voice_Telephone: 406-587-6964
      Contact_Electronic_Mail_Address: wurie@fs.fed.us
      Hours_of_Service: 8:00 - 4:30
  Native_Data_Set_Environment:
    Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 1; ESRI ArcCatalog 8.1.2.671

Data_Quality_Information:
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: Streamnet
          Title: Pacific Northwest River Reach Files
          Online_Linkage: <http://www.streamnet.org/pnwr/pnwrhome.html>
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: Montana Department of Fish Wildlife and Parks
          Title: Montana Fish Wildlife and Parks River Reach Files
          Online_Linkage: <http://fwp.state.mt.us/insidefwp/fwplibrary/gis>

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: String
      Point_and_Vector_Object_Count: 18417

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Map_Projection:
        Map_Projection_Name: Albers Conical Equal Area
        Albers_Conical_Equal_Area:
          Standard_Parallel: 29.500000
          Standard_Parallel: 45.500000
          Longitude_of_Central_Meridian: -96.000000
          Latitude_of_Projection_Origin: 23.000000
          False_Easting: 0.000000
          False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.002048
          Ordinate_Resolution: 0.002048
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: D_Clarke_1866
      Ellipsoid_Name: Clarke 1866
      Semi-major_Axis: 6378206.400000
      Denominator_of_Flattening_Ratio: 294.978698

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: westslope_rte
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: LLID
      Attribute_Definition:
        LLID - The latitude and longitude at the mouth of the stream. The LLID is used to uniquely identify each stream and to link to the MS Access database associated with the Westslope Cutthroat Range-wide Assessment
    Attribute:
      Attribute_Label: MILES
      Attribute_Definition: Miles: Stream length in miles
    Attribute:
      Attribute_Label: NAME
      Attribute_Definition: Name: Stream Name
    Attribute:
      Attribute_Label: BEGMEAS
      Attribute_Definition:
        BEGMEAS: The stream measure at the beginning (downstream end) of the route
    Attribute:
      Attribute_Label: ENDMEAS
      Attribute_Definition:
        ENDMEAS: The The stream measure at the end (upstream end) of the route

Distribution_Information:
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 49.655

Metadata_Reference_Information:
  Metadata_Date: 20030501
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Wendi Urie
        Contact_Organization: US Forest Service
      Contact_Address:
        Address_Type:
          REQUIRED: The mailing and/or physical address for the organization or individual.
        City: REQUIRED: The city of the address.
        State_or_Province: REQUIRED: The state or province of the address.
        Postal_Code: REQUIRED: The ZIP or other postal code of the address.
      Contact_Voice_Telephone: 406-587-6964
      Contact_Electronic_Mail_Address: wurie@fs.fed.us
      Hours_of_Service: 8:00 - 4:30
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.7.3 on Thu May 01 16:08:15 2003