Identification_Information:
  Citation:
    Citation_Information:
      Originator: StreamNet Project, Pacific States Marine Fisheries Commission
      Publication_Date: 20080723
      Title: StreamNet Mixed-Scale routed Hydrography (MSHv1- draft3)
      Geospatial_Data_Presentation_Form: vector digital data
      Publication_Information:
        Publication_Place: Portland, Oregon
        Publisher: StreamNet Project, Pacific States Marine Fisheries Commission
      Online_Linkage: http://www.streamnet.org/online-data/GISData.html
  Description:
    Abstract:
      This whole-stream routed hydrography layer serves as the base hydrography for the StreamNet project's Linear Referencing System (LRS). To distinguish this hydrography layer from the previous system(s), StreamNet refers to it as "MSHv1" (Mixed-scale hydrography, version 1).

      At version1: this dataset includes all routed streams present in the PNW River Reach Files (PNWRF3), StreamNet's previous base hydrography. In addition, those features within the state of Washington are now depicted at a higher resolution (24k scale) and densified to include all named streams present in Washington Department of Fish and Wildlife's 24k hydrography layer, and additional unnamed streams from that source where fish data exists and is compiled across the region. Future versions of this dataset will include similar improvements for StreamNet's other partner states (Oregon, Idaho, and Montana).  In addition, the extent of StreamNet's regional hydrography has expanded to include integration with the 1:100k scale routed hydrography for California (CalHydro).  While the StreamNet project does not manage fish data for California, the integration of California hydrography facilitates collaboration with StreamNet's partner project, "CalFISH".  For more information about the CalFISH project, visit http://www.CalFISH.org.  For more information about the source data contributing to this dataset, see the lineage section of this metadata record.
    Purpose: The primary purpose of this dataset is to provide a route system ideal for storing, organizing, and displaying stream related fisheries and habitat data across the Pacific Northwest and California at the best practically available source scale.  An on-going effort involves improving the resolution of the source datasets that makeup this regional layer.  In addition to providing a regionally standard LRS, the MSHv1 can support many different types of GIS analysis including: buffering around reaches, stream network routing, and basin characteristics analysis.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 20080723
    Currentness_Reference: publication date
  Status:
    Progress: In work
    Maintenance_and_Update_Frequency: As needed
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -126.093754
      East_Bounding_Coordinate: -108.586955
      North_Bounding_Coordinate: 52.130782
      South_Bounding_Coordinate: 32.294133
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: ESRI Geography Network Thesaurus
      Theme_Keyword: inlandWaters, hydrography, environment
    Place:
      Place_Keyword_Thesaurus: None
      Place_Keyword: Pacific Northwest, west coast, Columbia River Basin, Washington, Oregon, Idaho, Montana, California
  Access_Constraints: Public, Tribal Enterprises, Tribal Government, Individual Authorized Users
  Use_Constraints: None
  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
        Contact_Person: Van C. Hare
      Contact_Position: StreamNet Project, Regional GIS Manager
      Contact_Address:
        Address_Type: mailing
        Address: 205 SE Spokane Street, Suite 100
        City: Portland
        State_or_Province: OR
        Postal_Code: 97202
        Country: USA
      Contact_Voice_Telephone: 503-595-3155
      Contact_Facsimile_Telephone: 503-595-3232
      Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
      Hours_of_Service: Monday - Friday, 9am -5pm
      Contact_Instructions: Email is the preferred mode of contact.
  Data_Set_Credit: StreamNet Project, Pacific States Marine Fisheries Commission, Portland, Oregon
  Security_Information:
    Security_Classification_System: PSMFC
    Security_Classification: Level 1: Public
    Security_Handling_Description: Public data is accessible to all requester categories, including the General Public, with limited to no restrictions.
  Native_Data_Set_Environment: Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 3; ESRI ArcCatalog 9.2.4.1420
  Cross_Reference:
    Citation_Information:
      Publication_Information:
        Publication_Place: Portland, Oregon
        Publisher: StreamNet Project, Pacific States Marine Fisheries Commission
Data_Quality_Information:
  Logical_Consistency_Report: ESRI feature type: Simple, Geometry: Polyline, Topology:
  Completeness_Report: Data set has been visually inspected.  All data produced strives to meet National Mapping Accuracy Standards (NMAS).
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: StreamNet Project, Pacific States Marine Fisheries Commission
          Publication_Date: 20080423
          Title: PNW River Reach Files, 1:100k LLID Routed Streams
          Geospatial_Data_Presentation_Form: vector digital data
          Other_Citation_Details: Includes best available updates of the PNWRF3 obtained from StreamNet partner agencies in Oregon, Idaho and Montana. Updates from Montana were contributed as a measured shapefile, while Oregon and Idaho features were contributed as route features in an ArcInfo coverage.  Original arc attributes are archived but only route features exist in the MSHv1.
          Online_Linkage: http://www.StreamNet.org/online-data/GISData.html
      Source_Scale_Denominator: 1:100,000
      Type_of_Source_Media: online
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 20080423
        Source_Currentness_Reference: publication date
      Source_Citation_Abbreviation: PNWRF3
      Source_Contribution:
        Source linework and route attributes for hydrography features in Oregon, Idaho and western Montana.  Linework for mainstem rivers flowing into or from Canada was provided by IDFG as an enhancement to the original PNWRF3.  This source dataset served as the basis for referencing StreamNet data in the past (1997-2008).  It continues to be archived and will remain available online at http://www.streamnet.org/online-data/GISData.html. 

        Features from the best available version of this source were edgematched and appended together with a subset of WDFW's 24K Streams layer and the CalHydro dataset.  Finally, routes were merged and rebuilt where necessary and all whole-stream routes were remeasured. See process steps in the lineage section of this metadata record for more information.
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: Washington Department of Fish and Wildlife
          Publication_Date: 20070125
          Title: WDFW Mixed-scale hydrography, select 1:24k LLID routed streams
          Geospatial_Data_Presentation_Form: vector digital data
      Source_Scale_Denominator: 1:100,000
      Type_of_Source_Media: online
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 20080423
        Source_Currentness_Reference: publication date
      Source_Citation_Abbreviation: PNWRF3
      Source_Contribution:
        Source linework and route attributes for hydrography features in Oregon, Idaho and western Montana.  Linework for mainstem rivers flowing into or from Canada was provided by IDFG as an enhancement to the original PNWRF3.  This source dataset served as the basis for referencing StreamNet data in the past (1997-2008).  It continues to be archived and will remain available online at http://www.streamnet.org/online-data/GISData.html. 

        Features from the best available version of this source were edgematched and appended together with a subset of WDFW's 24K Streams layer and the CalHydro dataset.  Finally, routes were merged and rebuilt where necessary and all whole-stream routes were remeasured. See process steps in the lineage section of this metadata record for more information.
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: CalFISH project, California Dept. of Fish and Game and the Pacific States Marine Fisheries Commission
          Publication_Date: 20030915
          Title: CalHydro, 1:100k LLID routed streams
          Geospatial_Data_Presentation_Form: vector digital data
          Other_Citation_Details: Source data was a measured shapefile
          Online_Linkage: http://www.CalFISH.org
      Source_Scale_Denominator: 1:100,000
      Type_of_Source_Media: online
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 20080423
        Source_Currentness_Reference: publication date
      Source_Citation_Abbreviation: PNWRF3
      Source_Contribution:
        Source linework and route attributes for hydrography features in Oregon, Idaho and western Montana.  Linework for mainstem rivers flowing into or from Canada was provided by IDFG as an enhancement to the original PNWRF3.  This source dataset served as the basis for referencing StreamNet data in the past (1997-2008).  It continues to be archived and will remain available online at http://www.streamnet.org/online-data/GISData.html. 

        Features from the best available version of this source were edgematched and appended together with a subset of WDFW's 24K Streams layer and the CalHydro dataset.  Finally, routes were merged and rebuilt where necessary and all whole-stream routes were remeasured. See process steps in the lineage section of this metadata record for more information.
    Process_Step:
      Process_Description: Best available PNWRF3 datasets were collected and appended for Idaho, Oregon and western Montana.  The latest working copies of the PNWRF3 were obtained from StreamNet partners to capture mostly minor corrections that have been made through time and include them in the MSHv1.  Updates were received from IDFG (ArcInfo coverage, "idfg_snhydro") and MFWP (measured shapefile, "strm_rts").  Route features were appended for ID, MT and OR.  Attributes for BegFt and LengthFt were retained to maintain flow direction and permit the rebuilding of routes using the ArcGIS 'Create Routes' Linear Referencing Tool (which requires from-measure and to-measure fields).
      Source_Used_Citation_Abbreviation: PNWRF3
      Process_Date: 20080423
      Source_Produced_Citation_Abbreviation: ORIDMT
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
            Contact_Person: Van C. Hare
          Contact_Position: GIS Manager
          Contact_Voice_Telephone: 503-595-3100
          Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
          Hours_of_Service: Monday - Friday, 9am-5pm
          Contact_Instructions: Email is the preferred mode of contact
    Process_Step:
      Process_Description: Appended WDFW's "strmsh" dataset to the previously compiled PNWRF3 data.  Edgematched and merged routes where necessary and rebuilt routes using the ArcGIS 'Create Routes' Linear Referencing Tool (which requires from-measure and to-measure fields).
      Source_Used_Citation_Abbreviation: WDFW "strmsh" & ORIDMT
      Process_Date: 20080423
      Source_Produced_Citation_Abbreviation: ORIDMTWA
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
            Contact_Person: Van C. Hare
          Contact_Position: GIS Manager
          Contact_Voice_Telephone: 503-595-3100
          Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
          Hours_of_Service: Monday - Friday, 9am-5pm
          Contact_Instructions: Email is the preferred mode of contact
    Process_Step:
      Process_Description: Appended CalHydro dataset to output of process step 2. Edgematched and merged routes where necessary and rebuilt routes using the ArcGIS 'Create Routes' Linear Referencing Tool (which requires from-measure and to-measure fields). Note that areas of overlap exist between the PNWRF3 and CalHydro source datasets. Source features were selected based on the direction of flow within a HUC4.  Streams flowing south into California were pulled from the CalHydro dataset where possible and those flowing north into Oregon were sourced from the PNWRF3.  For the Klamath River, a source split was made at the outlet of Upper Klamath Lake. LLIDSRC and MEASSRC fields in the final product are useful for tracking the lineage of individual features.  After this final data source was integrated, all routes were remeasured based on the newly refreshed BegFt and LengthFt fields.  For the non-California sourced features, these measures are based on an integer version of the actual route lengths based on the MSHv1 projection (StreamNet Lambert, NAD83).  For the CalHydro sourced features, BegFt and LengthFt values remain based on the values present in the original source dataset (which was determined using California's Teale Albers projection, NAD83).  This was done purposefully to enable existing CalFISH event data to be mapped using the MSHv1 directly.
      Source_Used_Citation_Abbreviation: CalHydro (CDFG_100k_2003_6.shp) & ORIDMTWA
      Process_Date: 20080423
      Source_Produced_Citation_Abbreviation: MSHv1_pre
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
            Contact_Person: Van C. Hare
          Contact_Position: GIS Manager
          Contact_Address:
            Address_Type: mailing and physical address
          Contact_Voice_Telephone: 503-595-3100
          Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
          Hours_of_Service: Monday - Friday, 9am-5pm
          Contact_Instructions: Email is the preferred mode of contact
    Process_Step:
      Process_Description: Assign attributes and QC first draft dataset. The LLID field is used as a key to crosswalk and standardize feature attributes from the multiple sources. Included in this process was the addition of information about the logical stream network - assigning Tributary IDs and Names from existing tables managed by StreamNet partners and the regional office.  Additional fields used for internal QC routines were also added and populated as part of the review process. This first review included initial testing of the LRS by WDFW and ODFW
      Source_Used_Citation_Abbreviation: MSHv1_pre
      Process_Date: 20080423
      Source_Produced_Citation_Abbreviation: MSHv1 (first draft)
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
            Contact_Person: Van C. Hare
          Contact_Position: GIS Manager
          Contact_Voice_Telephone: 503-595-3100
          Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
          Hours_of_Service: Monday - Friday, 9am-5pm
          Contact_Instructions: Email is the preferred mode of contact
    Process_Step:
      Process_Description: Second draft review, included correction of some stream and tributary naming errors, merging of some route features, rebuilding and remeasuring of routes where necessary and additional QC commenting. This current version is under review for more thorough testing and migration of existing StreamNet LRS event tables.
      Source_Used_Citation_Abbreviation: MSHv1 (first draft)
      Process_Date: 20080423
      Source_Produced_Citation_Abbreviation: MSHv1 (second draft)
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
            Contact_Person: Van C. Hare
          Contact_Position: GIS Manager
          Contact_Voice_Telephone: 503-595-3100
          Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
          Hours_of_Service: Monday - Friday, 9am-5pm
          Contact_Instructions: Email is the preferred mode of contact
    Process_Step:
      Process_Description: Correction of issues identified in 2nd draft and improved attribution.  The main changes include QC of stream name and TribID information and remeasurement of a number of streams near the Oregon/California border.  These streams are readily identifiable by selecting GISHook = 42.  In draft 2 of this dataset, these streams were measured based on their CalHydro measure system (based on Teale Albers projection).  At draft 3, they  have been re-measured based on the StreamNet Lambert projection to minimize the impact on linear event data managed by ODFW.  Additional notes and internal codes to support QA/QC were also added at draft 3. In some cases these attributes will be stripped from the final publication datset.
      Source_Used_Citation_Abbreviation: MSHv1 (draft 2)
      Process_Date: 20080723
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
            Contact_Person: Van C. Hare
          Contact_Position: GIS Manager
          Contact_Voice_Telephone: 503-595-3155
          Contact_Facsimile_Telephone: 503-595-3232
          Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
          Hours_of_Service: Monday - Friday, 9am to 5pm
          Contact_Instructions: Email is the preferred mode of contact
    Process_Step:
      Process_Description: Metadata imported and modified from previous draft
      Process_Date: 20080723
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation: \\VAN-XP\Workspace\MSHv1_9_1.mdb
    Process_Step:
      Process_Description: Metadata imported.
      Source_Used_Citation_Abbreviation: O:\sde.DBO.MSHv1_draft3.xml
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation: Server=honu; Service=5151; Database=sde; User=sde_dbo; Version=sde.DEFAULT
Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: String
      Point_and_Vector_Object_Count: 152426
Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Map_Projection:
        Map_Projection_Name: Lambert Conformal Conic
        Lambert_Conformal_Conic:
          Standard_Parallel: 42.333333
          Standard_Parallel: 48.666667
          Longitude_of_Central_Meridian: -117.000000
          Latitude_of_Projection_Origin: 41.000000
          False_Easting: 2999999.999988
          False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.003511
          Ordinate_Resolution: 0.003511
        Planar_Distance_Units: survey feet
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222
  Vertical_Coordinate_System_Definition:
    Altitude_System_Definition:
      Altitude_Resolution: 1.000000
      Altitude_Encoding_Method: Explicit elevation coordinate included with horizontal coordinates
Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Hydrort_MSHv1_draft3
    Attribute:
      Attribute_Label: OBJECTID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: LLID
      Attribute_Definition: Unique whole stream identifier
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Unrepresentable_Domain: Unique stream identifier derived by concatenating the Longitude and Latitude coordinates of the stream mouth. Simply used as a unique ID.  Alias = LocationID
    Attribute:
      Attribute_Label: NAME
      Attribute_Definition: Stream name as identified by contributed sources
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Unrepresentable_Domain: Stream name as identified in source hydrography layer.  In cases where a stream is unnamed it is labeled "Unnamed Stream"
    Attribute:
      Attribute_Label: LENGTHFT
      Attribute_Definition: Length of stream in feet (integer) based on the projection system identified in the "MeasSrc" field
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 4
          Range_Domain_Maximum: 6431224
          Attribute_Units_of_Measure: Feet
          Attribute_Measurement_Resolution: 1
      Attribute_Value_Accuracy_Information:
        Attribute_Value_Accuracy: integer
        Attribute_Value_Accuracy_Explanation: rounded to the nearest integer based on the Shape.Length value for the feature or on the LengthFt measure defined by the source (in the case of CalHydro sourced features).
    Attribute:
      Attribute_Label: TRIBID
      Attribute_Definition: LLID (LocationID) for the waterbody the stream flows into. In addition to identifying the unique LLID for a downstream or 'parent' route, values include an enumerated domain of descriptive codes. The name or description relating to the TribID is carried in the TribToName field
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: -Unique 14 character LLID-
          Enumerated_Domain_Value_Definition: The LLID of the downstream waterbody the route flows into.  In cases where a distinct waterbody is not identified as being downstream, a codeset is used to generally describe flow.
        Enumerated_Domain:
          Enumerated_Domain_Value: 6000
          Enumerated_Domain_Value_Definition: Flows into Canada
        Enumerated_Domain:
          Enumerated_Domain_Value: 6001
          Enumerated_Domain_Value_Definition: Flows into California
        Enumerated_Domain:
          Enumerated_Domain_Value: 6002
          Enumerated_Domain_Value_Definition: Flows into Nevada
        Enumerated_Domain:
          Enumerated_Domain_Value: 6003
          Enumerated_Domain_Value_Definition: Flows into Utah
        Enumerated_Domain:
          Enumerated_Domain_Value: 6004
          Enumerated_Domain_Value_Definition: Flows into Wyoming
        Enumerated_Domain:
          Enumerated_Domain_Value: 6005
          Enumerated_Domain_Value_Definition: No outlet (stream goes subsurface)
        Enumerated_Domain:
          Enumerated_Domain_Value: 6006
          Enumerated_Domain_Value_Definition: Flows into unnamed 24k stream
        Enumerated_Domain:
          Enumerated_Domain_Value: 6007
          Enumerated_Domain_Value_Definition: Flows into Strait of Juan de Fuca
        Enumerated_Domain:
          Enumerated_Domain_Value: 6008
          Enumerated_Domain_Value_Definition: Flows into Hood Canal
        Enumerated_Domain:
          Enumerated_Domain_Value: 6009
          Enumerated_Domain_Value_Definition: Flows into Puget Sound
        Enumerated_Domain:
          Enumerated_Domain_Value: 6010
          Enumerated_Domain_Value_Definition: Flows into Wilapa Bay
        Enumerated_Domain:
          Enumerated_Domain_Value: 6011
          Enumerated_Domain_Value_Definition: Flows into Grays Harbor
        Enumerated_Domain:
          Enumerated_Domain_Value: 6012
          Enumerated_Domain_Value_Definition: Flows into Mexico
        Enumerated_Domain:
          Enumerated_Domain_Value: 6022
          Enumerated_Domain_Value_Definition: Udetermined outlet in California
        Enumerated_Domain:
          Enumerated_Domain_Value: 6023
          Enumerated_Domain_Value_Definition: Undetermined outlet in Idaho
        Enumerated_Domain:
          Enumerated_Domain_Value: 6024
          Enumerated_Domain_Value_Definition: Undetermined outlet in Oregon
        Enumerated_Domain:
          Enumerated_Domain_Value: 6025
          Enumerated_Domain_Value_Definition: Undetermined outlet in Washington
        Enumerated_Domain:
          Enumerated_Domain_Value: 6026
          Enumerated_Domain_Value_Definition: Undetermined outlet in Montana
        Enumerated_Domain:
          Enumerated_Domain_Value: 6027
          Enumerated_Domain_Value_Definition: Undetermined outlet in Nevada
        Enumerated_Domain:
          Enumerated_Domain_Value: 6028
          Enumerated_Domain_Value_Definition: Undetermined outlet in Utah
        Enumerated_Domain:
          Enumerated_Domain_Value: 6029
          Enumerated_Domain_Value_Definition: Undetermined outlet in Wyoming
        Enumerated_Domain:
          Enumerated_Domain_Value: 6032
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in California
        Enumerated_Domain:
          Enumerated_Domain_Value: 6033
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Idaho
        Enumerated_Domain:
          Enumerated_Domain_Value: 6034
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Oregon
        Enumerated_Domain:
          Enumerated_Domain_Value: 6035
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Washington
        Enumerated_Domain:
          Enumerated_Domain_Value: 6036
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Montana
        Enumerated_Domain:
          Enumerated_Domain_Value: 6037
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Nevada
        Enumerated_Domain:
          Enumerated_Domain_Value: 6038
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Utah
        Enumerated_Domain:
          Enumerated_Domain_Value: 6039
          Enumerated_Domain_Value_Definition: Undetermined canal/pipeline in Wyoming
        Enumerated_Domain:
          Enumerated_Domain_Value: 1242091436511
          Enumerated_Domain_Value_Definition: Pacific Ocean
        Enumerated_Domain:
          Enumerated_Domain_Value: 1242091436512
          Enumerated_Domain_Value_Definition: Pacific Ocean off California
        Enumerated_Domain:
          Enumerated_Domain_Value: 1242091436514
          Enumerated_Domain_Value_Definition: Pacific Ocean off Oregon
        Enumerated_Domain:
          Enumerated_Domain_Value: 1242091436515
          Enumerated_Domain_Value_Definition: Pacific Ocean off Washington
    Attribute:
      Attribute_Label: TRIBTONAME
      Attribute_Definition: Name of stream or waterbody the route flows into - this is determined based on the TribID field
      Attribute_Domain_Values:
        Unrepresentable_Domain: Name of the stream or waterbody that the route flows into as identified in source hydrography layer.  In cases where a "tributary to" stream is unnamed it is labeled "Unnamed Stream [LLID]"
    Attribute:
      Attribute_Label: TRIBFT
      Attribute_Definition: Identifies the measured location of the confluence of the stream with its downstream parent.  When the TribToID identifies a routed stream, this field carries the measure (in feet) that locates the point of confluence of this route with its downstream parent. This field is left blank if the stream does not flow into another routed feature.
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Unrepresentable_Domain: Unique identifier of the downstream feature
    Attribute:
      Attribute_Label: XREFNAME
      Attribute_Definition: A descriptive, qualified stream name derived from a combination of NAME and TRIBTONAME
    Attribute:
      Attribute_Label: SNWEBLINK
      Attribute_Definition: A hyperlink constructed to return a summary report of data available in the StreamNet Web Query System referenced to the route based on its unique LLID (LocationID).  This field can be used to link directly to StreamNet via the identify tool in ArcGIS or set as the hyperlink field for use with the ArcGIS hyperlink tool.
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Unrepresentable_Domain: Uniquely constructed hyperlink to retrieve fish data based on LLID
    Attribute:
      Attribute_Label: FEATURE
      Attribute_Definition: Feature type description used to distinguish watercourse from coastline features
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: Coastline
          Enumerated_Domain_Value_Definition: Coastline features - these are not currently used by StreamNet to carry event data but may be in the future.  A public distribution of the Hydrography may exclude these features
        Enumerated_Domain:
          Enumerated_Domain_Value: Watercourse
          Enumerated_Domain_Value_Definition: Watercourse features - includes streams, ditches, canals and pipeline features. LOCTYPE and LOCSUBTYPE fields may be used to further separate out the different types of watercourse features.
    Attribute:
      Attribute_Label: LOCTYPE
      Attribute_Definition: INTERNAL - Used to facilitate synching between tabular database and GIS.  Field will be excluded in the published version of this dataset
      Attribute_Definition_Source: StreamNet LOCMASTER Table
    Attribute:
      Attribute_Label: LOCSUBTYPE
      Attribute_Definition: INTERNAL - As values in this field become more complete, subtype descriptions may be incorporated into the FEATURE field.  Currently this is used internally to synch the GIS with StreamNet's tabular database. More work is necessary to accurately identify ditch/canal/pipeline features
      Attribute_Definition_Source: StreamNet LOCMASTER Table
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 100
          Enumerated_Domain_Value_Definition: 100k stream
        Enumerated_Domain:
          Enumerated_Domain_Value: 110
          Enumerated_Domain_Value_Definition: 100k ditch/canal/pipeline
        Enumerated_Domain:
          Enumerated_Domain_Value: 120
          Enumerated_Domain_Value_Definition: 24k stream
        Enumerated_Domain:
          Enumerated_Domain_Value: 130
          Enumerated_Domain_Value_Definition: 24k ditch/canal/pipeline
        Enumerated_Domain:
          Enumerated_Domain_Value: 140
          Enumerated_Domain_Value_Definition: 100k coastline feature
    Attribute:
      Attribute_Label: OLDMAXMEAS
      Attribute_Definition: INTERNAL - This field contains the previous length measure (maxm) associated with an LLID in cases where the LLID existed in the StreamNet database prior to adoption of the MSHv1.  Field will be excluded in the published version of this dataset.
    Attribute:
      Attribute_Label: MAXMEASDIF
      Attribute_Definition: INTERNAL - Values in this field represent the change in measure associated with an LLID. It was derived by subtracting the Shape.length value from the OLDMAXMEAS value.  This is useful for QC purposes to flag cases when a significant change in route length occured. Where this is the case, see the GISCOMMENT field for a description / explanation of what caused the change in length.  Where the LLID is new to the StreamNet database, this field will be null. Field will be excluded in the published version of this dataset.
    Attribute:
      Attribute_Label: MEASSRC
      Attribute_Definition: Feature level description of measurement source used to define the given routes measure system
      Attribute_Definition_Source: http://www.StreamNet.org
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: MSHv1.0 (SN Lambert Ft)
          Enumerated_Domain_Value_Definition: measures are based on the StreamNet Lambert Projection (NAD83) updated at creation of MSHv1
        Enumerated_Domain:
          Enumerated_Domain_Value: CalHydro 100k (Teale Albers Ft)
          Enumerated_Domain_Value_Definition: route measure is calibrated based on the original LenghtFt value contained in the CalHydro dataset. This value was originally based on the Teale Albers projection (ft) so the measures for these routes will differ from the Shape.len value for the route.
    Attribute:
      Attribute_Label: LLIDSRC
      Attribute_Definition: Tracks the origin of the assigned LLID
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: PNWRF3 (100k)
          Enumerated_Domain_Value_Definition: LLID originates from the PNWRF3 dataset
        Enumerated_Domain:
          Enumerated_Domain_Value: CalHydro (100k)
          Enumerated_Domain_Value_Definition: LLID originates from the CalHydro dataset
        Enumerated_Domain:
          Enumerated_Domain_Value: WDFW MSHD (24k)
          Enumerated_Domain_Value_Definition: LLID originates from the WDFW mixed-scale hydrography dataset. These are newly assigned LLIDs that did not previously exist in the regional StreamNet database.  As they were assigned by WDFW internally, they may differ from another source's LLID for the same stream (e.g., PNW Framework Hydrography).
        Enumerated_Domain:
          Enumerated_Domain_Value: MFWP NHD (100k)
          Enumerated_Domain_Value_Definition: LLID assigned by MFWP for a 100k stream not originally routed in the PNWRF3 dataset (linework pulled from 100k NHD)
        Enumerated_Domain:
          Enumerated_Domain_Value: MFWP (24k)
          Enumerated_Domain_Value_Definition: LLID assigned by MFWP for a 24k stream not originally in the PNWRF3 dataset (linework digitized by MFWP at 1:24k scale)
    Attribute:
      Attribute_Label: GISHOOK
      Attribute_Definition: INTERNAL - Used by GIS staff to categorize features for QA/QC.  Field will be excluded from the published version of this dataset.  A layer file is available to help StreamNet Staff use this field (Hydrort_MSHv1_GISHook.lyr). Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: StreamNet Regional GIS
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 20
          Enumerated_Domain_Value_Definition: CA: Original Calhydro
        Enumerated_Domain:
          Enumerated_Domain_Value: 26
          Enumerated_Domain_Value_Definition: CA: Cross-border stream, defer to CA
        Enumerated_Domain:
          Enumerated_Domain_Value: 30
          Enumerated_Domain_Value_Definition: ID: Original PNWRF3
        Enumerated_Domain:
          Enumerated_Domain_Value: 32
          Enumerated_Domain_Value_Definition: ID: New/edited since PNWRF3
        Enumerated_Domain:
          Enumerated_Domain_Value: 35
          Enumerated_Domain_Value_Definition: ID: See ToDo Comment
        Enumerated_Domain:
          Enumerated_Domain_Value: 36
          Enumerated_Domain_Value_Definition: ID: Cross-border stream, defer to ID
        Enumerated_Domain:
          Enumerated_Domain_Value: 37
          Enumerated_Domain_Value_Definition: ID: Cross-border stream, partially coincident with border
        Enumerated_Domain:
          Enumerated_Domain_Value: 40
          Enumerated_Domain_Value_Definition: OR: Original PNWRF3
        Enumerated_Domain:
          Enumerated_Domain_Value: 42
          Enumerated_Domain_Value_Definition: OR: Remeasured Edited or New 100k
        Enumerated_Domain:
          Enumerated_Domain_Value: 44
          Enumerated_Domain_Value_Definition: OR: MSH New 24k addition
        Enumerated_Domain:
          Enumerated_Domain_Value: 45
          Enumerated_Domain_Value_Definition: OR: See ToDo Comments
        Enumerated_Domain:
          Enumerated_Domain_Value: 46
          Enumerated_Domain_Value_Definition: OR: Cross-border stream, defer to OR
        Enumerated_Domain:
          Enumerated_Domain_Value: 49
          Enumerated_Domain_Value_Definition: OR: Coastline
        Enumerated_Domain:
          Enumerated_Domain_Value: 52
          Enumerated_Domain_Value_Definition: WA: MSH 100k streams
        Enumerated_Domain:
          Enumerated_Domain_Value: 54
          Enumerated_Domain_Value_Definition: WA: MSH New 24k additions
        Enumerated_Domain:
          Enumerated_Domain_Value: 55
          Enumerated_Domain_Value_Definition: WA: See ToDo Comments
        Enumerated_Domain:
          Enumerated_Domain_Value: 56
          Enumerated_Domain_Value_Definition: WA: Cross-border stream, defer to WA
        Enumerated_Domain:
          Enumerated_Domain_Value: 57
          Enumerated_Domain_Value_Definition: WA: Cross-border stream, partially coincident with state border
        Enumerated_Domain:
          Enumerated_Domain_Value: 60
          Enumerated_Domain_Value_Definition: MT: Original PNWRF3
        Enumerated_Domain:
          Enumerated_Domain_Value: 62
          Enumerated_Domain_Value_Definition: MT: New/edited since PNWRF3
        Enumerated_Domain:
          Enumerated_Domain_Value: 65
          Enumerated_Domain_Value_Definition: MT: See ToDo Comments
        Enumerated_Domain:
          Enumerated_Domain_Value: 66
          Enumerated_Domain_Value_Definition: MT: Cross-border stream, defer to MT
        Enumerated_Domain:
          Enumerated_Domain_Value: 70
          Enumerated_Domain_Value_Definition: BC: MSH 100k (IDFG sourced)
    Attribute:
      Attribute_Label: GISSYNCH
      Attribute_Definition: INTERNAL - Used by GIS staff. Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: StreamNet Regional GIS
    Attribute:
      Attribute_Label: GISNOTE
      Attribute_Definition: INTERNAL - Used by GIS staff to document notes related to QA/QC of GIS dataset.  Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: StreamNet Regional GIS
    Attribute:
      Attribute_Label: WACOMMENTS
      Attribute_Definition: INTERNAL - Used by WDFW staff to record LocationID comments related to MSH migration.  Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: StreamNet WDFW staff
    Attribute:
      Attribute_Label: COMMENTS
      Attribute_Definition: INTERNAL - Used by StreamNet PSMFC staff to document notes related to QA/QC of tabular dataset.  Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: StreamNet PSMFC staff
    Attribute:
      Attribute_Label: INDATA
      Attribute_Definition: INTERNAL - Count used to identify the number of data categories a LocationID is referenced in (as of GISSynch date). Van and Bill use this field during QC for prioritizing the resolution of location related issues. Field will be excluded in the published version of this dataset. INTERNAL - Used by GIS staff to document notes related to QA/QC of GIS dataset.  Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: LOCMASTERXTALLY
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 0
          Range_Domain_Maximum: 10
    Attribute:
      Attribute_Label: INCRB
      Attribute_Definition: INTERNAL - Flags routes that are contained within the Columbia River Basin. Van and Bill use for QC. Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: LOCMASTERXTALLY
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 0
          Enumerated_Domain_Value_Definition: route does not lay within the Columbia Basin
        Enumerated_Domain:
          Enumerated_Domain_Value: 1
          Enumerated_Domain_Value_Definition: route does lay within the Columbia Basin
    Attribute:
      Attribute_Label: INCAL
      Attribute_Definition: INTERNAL - Flags streams that lay within California. Van and Bill use for QC. Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: LOCMASTERXTALLY
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 0
          Enumerated_Domain_Value_Definition: route is not in California
        Enumerated_Domain:
          Enumerated_Domain_Value: 1
          Enumerated_Domain_Value_Definition: route is in California
    Attribute:
      Attribute_Label: NOCOREGHUC
      Attribute_Definition: INTERNAL - Flags streams that will not logically be present in LOCX tables for COUNTY, REGION, or HUC.  These are largely spatially ambiguous supercodes or coastline features, etc. Van and Bill use for QC. Field will be excluded in the published version of this dataset.
      Attribute_Definition_Source: LOCMASTERXTALLY
    Attribute:
      Attribute_Label: SHAPE
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: SHAPE_Length
      Attribute_Definition: Length of feature in internal units.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
  Overview_Description:
Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
        Contact_Person: Van C. Hare
      Contact_Position: StreamNet Project, Regional GIS Manager
      Contact_Address:
        Address_Type: mailing
        Address: 205 SE Spokane Street, Suite 100
        City: Portland
        State_or_Province: OR
        Postal_Code: 97202
        Country: USA
      Contact_Voice_Telephone: 503-595-3155
      Contact_Facsimile_Telephone: 503-595-3232
      Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
      Hours_of_Service: Monday - Friday, 9am -5pm
      Contact_Instructions: Email is the preferred mode of contact.
  Resource_Description: Downloadable Data
  Distribution_Liability: None
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ESRI data format, dependent upon request
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name: http://www.streamnet.org/online-data/GISData.html
    Fees: To be determined at time of order
Metadata_Reference_Information:
  Metadata_Date: 20080822
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: StreamNet Project, Pacific States Marine Fisheries Commission
        Contact_Person: Van C. Hare
      Contact_Position: StreamNet Project, Regional GIS Manager
      Contact_Address:
        Address_Type: mailing
        Address: 205 SE Spokane Street, Suite 100
        City: Portland
        State_or_Province: OR
        Postal_Code: 97202
        Country: USA
      Contact_Voice_Telephone: 503-595-3155
      Contact_Facsimile_Telephone: 503-595-3232
      Contact_Electronic_Mail_Address: StreamNetGIS@psmfc.org
      Hours_of_Service: Monday - Friday, 9am -5pm
      Contact_Instructions: Email is the preferred mode of contact.
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Security_Information:
    Metadata_Security_Classification: Unclassified
  Metadata_Extensions:
    Online_Linkage: http://www.esri.com/metadata/esriprof80.html
    Profile_Name: ESRI Metadata Profile
