106	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	160	9	31
107	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	161	9	32
132	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	186	9	62
133	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	187	9	101
134	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	188	9	102
135	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	189	9	141
136	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	190	9	142
137	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	191	9	162
138	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	192	9	31
139	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	193	9	32
140	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	194	9	61
141	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	195	9	62
142	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	196	9	101
143	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	197	9	102
144	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	198	9	141
145	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	199	9	142
108	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	162	9	61
109	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	163	9	62
110	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	164	9	101
111	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	165	9	102
112	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	166	9	141
113	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	167	9	142
114	Chilliwist 6 Waterfall				Chilliwist 6 Diversion Waterfall, Upstream 9 lowest 66 percent no pattern.  Use .66 in all months	Chilliwist 6 Diversion falls dam (Stan Stout) All Waterfall Upstream all 0 NA 1 SSHEAR	1	23	168	9	162
115	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	169	9	31
116	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	170	9	32
117	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	171	9	61
118	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	172	9	62
119	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	173	9	101
120	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	174	9	102
121	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	175	9	141
122	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	176	9	142
123	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	177	9	162
124	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	178	1	31
125	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	179	1	5
146	Chilliwist 4				Culvert barrier for steelhead at Age 0 and Age 1 (fingerling and juvenille)  pattern No. 1	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	17	200	9	162
147	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	201	9	31
166	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	220	9	32
167	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	221	9	61
168	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	222	9	62
169	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	223	9	101
170	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	224	9	102
171	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	225	9	141
172	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	226	9	142
173	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	227	9	162
174	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	228	9	31
175	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	229	9	32
176	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	230	9	61
177	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	231	9	62
178	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	232	9	101
179	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	233	9	102
180	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	234	9	141
181	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	235	9	142
148	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	202	9	32
149	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	203	9	61
150	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	204	9	62
151	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	205	9	101
152	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	206	9	102
153	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	207	9	141
154	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	208	9	142
155	Chilliwist 4				Culvert barrier to Age 0 and Age 1 (fingerling and juvenille) steelhead.  Not a barrier for template.	c Upstream 9 lowest 66 1 1 SSHEAR; HWG	3	18	209	9	162
156	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	210	9	31
157	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	211	9	32
158	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	212	9	61
159	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	213	9	62
160	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	214	9	101
161	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	215	9	102
162	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	216	9	141
163	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	217	9	142
164	Loup Loup 2 Culvert				Loup Loup 2 Culvert Barrier Age-0 c Upstream  all 0      No pattern.  Use .66 for all months for upstream		3	31	218	9	162
165	Loup Loup 4 Culvert				At Hwy 97.  Loup Loup 4 Culvert Barrier 2 Hwy 97 Age-0 c Upstream  all 0 NA 1 SSHEAR; HWG.  No pattern available.  Use .66 for all 0 age migrants (fingerling)		3	37	219	9	31
126	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	180	1	61
127	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	181	1	101
182	Loup Loup 6				Loup Loup 6 Diversion dam (Ralston) Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  Use pattern No. 5 for fingerling		4	43	236	9	162
183	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	237	9	31
204	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	258	9	62
205	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	259	9	101
206	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	260	9	102
207	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	261	9	141
208	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	262	9	142
209	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	263	9	162
219	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	273	1	31
220	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	274	1	5
221	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	275	1	61
184	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	238	9	32
185	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	239	9	61
186	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	240	9	62
187	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	241	9	101
188	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	242	9	102
189	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	243	9	141
190	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	244	9	142
191	Loup Loup 8 Falls				Loup Loup 8 falls Age-0 fingerling Waterfall Upstream all 0 NA 1 LFA, HWG.  No pattern available.  Use .66 in all months for fingerling		1	49	245	9	162
192	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	246	9	31
193	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	247	9	32
194	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	248	9	61
195	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	249	9	62
196	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	250	9	101
197	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	251	9	102
198	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	252	9	141
199	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	253	9	142
200	Loup Loup 10 (irrigation Diversion				Loup Loup 10 Leader Lake Diverson Age-0 fingerling Irrigation Diversion Upstream  7-9 0 5  LFA, HWG  John Arterburn will check on the months that it operates?  Use pattern No. 5 provincially for fingerlings		4	55	254	9	162
201	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	255	9	31
202	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	256	9	32
203	Tallant 2 Culvert				Tallant 2 Old Hwy 97 culvert ??       Casey will look at it?   No data.  Assume .66 for all months for fingerlings		3	63	257	9	61
128	Chilliwist 2 culvert				Chiliwist 2 OBS.  Steelhead barrier for Age 0 and Age 1.  Pattern No. 4	Chilliwist 2 Chiliwist 2 OBS Age-0 c Upstream 3 highest 66 SSHEAR; HWG    Age-1 c Upstream 3 highest 66 SSHEAR; HWG	3	11	182	1	162
129	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	183	9	31
223	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	277	1	162
222	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	276	1	101
246	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	300	1	162
252	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	306	9	31
253	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	307	9	32
254	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	308	9	61
255	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	309	9	62
256	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	310	9	101
224	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	278	9	31
225	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	279	9	32
226	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	280	9	61
227	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	281	9	62
228	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	282	9	101
229	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	283	9	102
230	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	284	9	141
231	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	285	9	142
232	Salmon 1a Alluvial fan				Salm1a alluvial fan at the mouth Age-0 fingerling Waterfall/alluvial fan Upstream all 0  1 BPA EIS draft, NRCS survey 1999, Entrix report 2000no historic barrier due to inundation by high Okanogan flows. Use Pattern No. 10		5	77	286	9	162
233	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	287	9	31
234	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	288	9	32
235	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	289	9	61
236	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	290	9	62
237	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	291	9	101
238	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	292	9	102
239	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	293	9	141
240	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	294	9	142
241	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	295	9	162
242	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	296	1	31
243	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	297	1	5
257	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	311	9	102
258	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	312	9	141
279	Omak 3h hatchery relaase point				Not an obstruction			145	333	1	162
280	Omak 3h hatchery relaase point				Not an obstruction			145	334	9	31
281	Omak 3h hatchery relaase point				Not an obstruction			145	335	9	32
282	Omak 3h hatchery relaase point				Not an obstruction			145	336	9	61
283	Omak 3h hatchery relaase point				Not an obstruction			145	337	9	62
284	Omak 3h hatchery relaase point				Not an obstruction			145	338	9	101
285	Omak 3h hatchery relaase point				Not an obstruction			145	339	9	102
286	Omak 3h hatchery relaase point				Not an obstruction			145	340	9	141
287	Omak 3h hatchery relaase point				Not an obstruction			145	341	9	142
288	Omak 3h hatchery relaase point				Not an obstruction			145	342	9	162
289	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	343	9	31
290	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	344	9	32
291	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	345	9	61
292	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	346	9	62
293	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	347	9	101
294	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	348	9	102
295	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	349	9	141
296	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	350	9	142
297	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	351	9	162
298	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	352	1	31
299	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	353	1	5
259	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	313	9	142
260	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	314	9	162
261	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	315	1	31
262	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	316	1	5
263	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	317	1	61
264	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	318	1	101
265	Salmon 11 Dam				Salm 11 Conconully Dam Age-0 fingerling Dam Upstream all 0 NA 1 LFA, HWG		2	103	319	1	162
266	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	320	9	31
267	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	321	9	32
268	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	322	9	61
269	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	323	9	62
270	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	324	9	101
271	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	325	9	102
272	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	326	9	141
273	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	327	9	142
274	SF Salm 2 Culvert				SFSalm 2 Full culvert barrier Age-0 fingerling Culvert Upstream all 0 NA 1 DNR (from SHEAPP database 2003)   No pattern defined, so assume 0 passage  for steelhead and sp chinook since they are currently blocked by downstream dam		3	115	328	9	162
275	Omak 3h hatchery relaase point				Not an obstruction			145	329	1	31
301	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	355	1	101
300	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	354	1	61
328	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	382	9	142
329	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	383	9	162
330	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	384	9	31
331	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	385	9	32
332	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	386	9	61
333	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	387	9	62
334	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	388	9	101
335	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	389	9	102
336	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	390	9	141
337	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	391	9	142
338	Omak 12 culvert				Omak 12 1st and 2nd culverts Age-0 fingerling Culvert Upstream high 66		3	183	392	9	162
339	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	393	9	31
340	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	394	9	32
341	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	395	9	61
342	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	396	9	62
343	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	397	9	101
344	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	398	9	102
345	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	399	9	141
346	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	400	9	142
347	Trail 2 Culvert				Trail 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0		3	191	401	9	162
348	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	402	9	31
349	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	403	9	32
350	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	404	9	61
351	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	405	9	62
352	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	406	9	101
353	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	407	9	102
354	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	408	9	141
355	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	409	9	142
356	Wannacut 2 Culvert				Wannacut 2 Possible road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	203	410	9	162
357	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	411	9	31
358	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	412	9	32
359	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	413	9	61
360	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	414	9	62
361	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	415	9	101
362	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	416	9	102
363	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	417	9	141
364	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	418	9	142
365	Wannacut 4 Culvert				Wannacut 4 Next road culvert All Culvert Upstream all 0 NA  LFA says no distribution past potential barriers; no surveys available		3	209	419	9	162
366	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	420	9	31
367	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	421	9	32
368	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	422	9	61
369	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	423	9	62
370	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	424	9	101
371	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	425	9	102
372	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	426	9	141
373	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	427	9	142
374	Tunk 2 Culvert				no information on this culvert.  Assume 100 percent passage until verified and pattern established.		3	221	428	9	162
384	Okanogna 22h hatchery release				no barrier			247	438	9	31
385	Okanogna 22h hatchery release				no barrier			247	439	9	32
386	Okanogna 22h hatchery release				no barrier			247	440	9	61
387	Okanogna 22h hatchery release				no barrier			247	441	9	62
388	Okanogna 22h hatchery release				no barrier			247	442	9	101
389	Okanogna 22h hatchery release				no barrier			247	443	9	102
390	Okanogna 22h hatchery release				no barrier			247	444	9	141
391	Okanogna 22h hatchery release				no barrier			247	445	9	142
392	Okanogna 22h hatchery release				no barrier			247	446	9	162
393	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	447	9	31
394	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	448	9	32
395	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	449	9	61
396	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	450	9	62
397	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	451	9	101
398	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	452	9	102
399	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	453	9	141
400	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	454	9	142
401	Aeanas 2				Aeanas 2 Culvert at Hwy 7 crossing (presumed dist.) Age-0 fingerling Culvert Upstream all 0 NA		3	241	455	9	162
402	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	456	9	31
403	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	457	9	32
404	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	458	9	61
405	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	459	9	62
406	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	460	9	101
407	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	461	9	102
408	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	462	9	141
409	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	463	9	142
410	Boneparte 2 Falls				Bonaparte 2 Barrier 5225 feet upstream all falls Upstream all 0 na		1	255	464	9	162
411	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	465	9	31
412	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	466	9	32
413	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	467	9	61
414	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	468	9	62
415	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	469	9	101
416	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	470	9	102
417	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	471	9	141
418	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	472	9	142
419	Whitestone 2 culvert				Whitestone 2 Barrier (culvert?) at River Loop Road all Culvert Upstream all 0 na  OCD -4 barriers between first unknown and Loomis Rd.		3	277	473	9	162
420	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	474	9	31
421	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	475	9	32
422	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	476	9	61
423	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	477	9	62
424	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	478	9	101
425	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	479	9	102
426	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	480	9	141
427	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	481	9	142
428	Whitestone 4 culvert				Whitestone 4 Barrier at Loomis Oroville Road Age-0 fingerling Culvert Upstream all 0 NA  OCD report 2003		3	283	482	9	162
429	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	483	9	31
430	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	484	9	32
431	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	485	9	61
432	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	486	9	62
433	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	487	9	101
434	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	488	9	102
435	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	489	9	141
436	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	490	9	142
437	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	491	9	162
438	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	492	1	31
439	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	493	1	5
440	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	494	1	61
441	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	495	1	101
442	Similkameen 6 Falls				Similkameen 6 Enloe Falls all falls upstream all 0 na		1	313	496	1	162
443	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	497	9	31
444	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	498	9	32
445	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	499	9	61
446	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	500	9	62
447	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	501	9	101
448	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	502	9	102
449	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	503	9	141
450	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	504	9	142
451	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	505	9	162
452	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	506	1	31
453	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	507	1	5
454	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	508	1	61
455	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	509	1	101
456	Similkameen 8 Dam				Similkameen 8 Enloe Dam all Dam upstream all 0 na		2	319	510	1	162
457	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	511	9	31
458	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	512	9	32
459	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	513	9	61
460	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	514	9	62
461	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	515	9	101
462	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	516	9	102
463	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	517	9	141
464	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	518	9	142
465	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	519	9	162
466	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	520	1	31
467	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	521	1	5
468	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	522	1	61
469	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	523	1	101
470	Zosel Dam				Okanogan 30 Zosel Dam Age-0 fingerling Dam Downstream 2 highest 85 9      Age-1 Juvenile Dam Downstream 2 highest 85 9      Adult Dam Upstream all 60 na  attraction efficiency to the ladders is an issue		2	339	524	1	162
471	Inkaneep Falls				Natural barrier at		1	43861	545	9	31
472	Inkaneep Falls				Natural barrier at		1	43861	546	9	32
473	Inkaneep Falls				Natural barrier at		1	43861	547	9	61
474	Inkaneep Falls				Natural barrier at		1	43861	548	9	62
475	Inkaneep Falls				Natural barrier at		1	43861	549	9	101
476	Inkaneep Falls				Natural barrier at		1	43861	550	9	102
477	Inkaneep Falls				Natural barrier at		1	43861	551	9	141
478	Inkaneep Falls				Natural barrier at		1	43861	552	9	142
479	Inkaneep Falls				Natural barrier at		1	43861	553	9	162
480	Inkaneep Falls				Natural barrier at		1	43861	554	1	31
481	Inkaneep Falls				Natural barrier at		1	43861	555	1	5
482	Inkaneep Falls				Natural barrier at		1	43861	556	1	61
483	Inkaneep Falls				Natural barrier at		1	43861	557	1	101
484	Inkaneep Falls				Natural barrier at		1	43861	558	1	162
485	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	559	1	31
486	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	560	1	5
487	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	561	1	61
488	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	562	1	101
489	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	563	1	162
490	Skaha Lake Dam				Historic falls on L bank (removed in 1910)	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43933	564	1	31
491	Skaha Lake Dam				Historic falls on L bank (removed in 1910)	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43933	565	1	5
492	Skaha Lake Dam				Historic falls on L bank (removed in 1910)	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43933	566	1	61
493	Skaha Lake Dam				Historic falls on L bank (removed in 1910)	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43933	567	1	101
494	Skaha Lake Dam				Historic falls on L bank (removed in 1910)	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43933	568	1	162
495	Okanagan Lake Dam				Same as Skaha Lake Dam	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43937	569	1	31
496	Okanagan Lake Dam				Same as Skaha Lake Dam	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43937	570	1	5
497	Okanagan Lake Dam				Same as Skaha Lake Dam	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43937	571	1	61
498	Okanagan Lake Dam				Same as Skaha Lake Dam	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43937	572	1	101
499	Okanagan Lake Dam				Same as Skaha Lake Dam	Knife gates.  Ladder is not used, likely not very effective due to disrepair.  Rated as no passage,but this is due to McIntrye dam blocking all anadromy.  If andromous fish encounter dam, passage would likely be zero or minimal due to dam confituration.	2	43937	573	1	162
500	Shingle Creek Dam				Channel spanning 4 foot high concrete.  At Rkm 1.2	This is a irrigation diversion.  Old and in disrepair.  Poorly designed fishway.	4	43941	574	1	31
501	Shingle Creek Dam				Channel spanning 4 foot high concrete.  At Rkm 1.2	This is a irrigation diversion.  Old and in disrepair.  Poorly designed fishway.	4	43941	575	1	5
502	Shingle Creek Dam				Channel spanning 4 foot high concrete.  At Rkm 1.2	This is a irrigation diversion.  Old and in disrepair.  Poorly designed fishway.	4	43941	576	1	61
503	Shingle Creek Dam				Channel spanning 4 foot high concrete.  At Rkm 1.2	This is a irrigation diversion.  Old and in disrepair.  Poorly designed fishway.	4	43941	577	1	101
504	Shingle Creek Dam				Channel spanning 4 foot high concrete.  At Rkm 1.2	This is a irrigation diversion.  Old and in disrepair.  Poorly designed fishway.	4	43941	578	1	162
505	McIntyre Dam				Channel spanning dam.  Knife gates.  Passage possible if gate operations were condtioned for fish passage.		4	43927	579	1	31
506	McIntyre Dam				Channel spanning dam.  Knife gates.  Passage possible if gate operations were condtioned for fish passage.		4	43927	580	1	5
507	McIntyre Dam				Channel spanning dam.  Knife gates.  Passage possible if gate operations were condtioned for fish passage.		4	43927	581	1	61
508	McIntyre Dam				Channel spanning dam.  Knife gates.  Passage possible if gate operations were condtioned for fish passage.		4	43927	582	1	101
509	McIntyre Dam				Channel spanning dam.  Knife gates.  Passage possible if gate operations were condtioned for fish passage.		4	43927	583	1	162
510	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	584	9	31
511	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	585	9	32
512	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	586	9	61
513	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	587	9	62
514	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	588	9	101
515	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	589	9	102
516	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	590	9	141
517	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	591	9	142
518	Vertical Drop Structures				Grade control structures in Mainstem Okanagan	These are channel spanning grade control structures.   Concrete apron in stream bed with no gates or ladders but there are overhead walkways necssitating .  There are 15 identical with No 1 and 12 having a different design in reaches (Canada numbers) 1-24.  2-11 and 13-17 will be rated or passage identically.  1 and 12 will have differenent assumptions. Engineering modeling identifed inpedence at high flow (~1000 cfs).		43865	592	9	162
302	Omak falls at Mission				Omak 5 Mission Falls Age-0 fingerling Waterfall Upstream all 0 NA		1	151	356	1	162
312	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	366	9	31
313	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	367	9	32
314	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	368	9	61
315	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	369	9	62
316	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	370	9	101
317	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	371	9	102
318	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	372	9	141
319	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	373	9	142
320	Swimpkin 2 Culvert				Swim 2 Hwy 155 barrier Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003		3	175	374	9	162
321	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	375	9	31
322	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	376	9	32
323	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	377	9	61
324	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	378	9	62
325	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	379	9	101
326	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	380	9	102
327	Stappaloop 2 culvert					Stap 2 Barrier at Hwy 155 Age-0 fingerling Culvert Upstream all 0 NA 1 SSHIAP database 2003	3	165	381	9	141
276	Omak 3h hatchery relaase point				Not an obstruction			145	330	1	5
277	Omak 3h hatchery relaase point				Not an obstruction			145	331	1	61
278	Omak 3h hatchery relaase point				Not an obstruction			145	332	1	101
244	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	298	1	61
245	Salmon 5 Diversion				Salm 5 OID Diversion  NA see notes     1 ladder and fish screens are in place so its not a barrier.  It dewaters the lower reaches during irrigation.		4	89	299	1	101
130	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	184	9	32
131	Chiliwist 2				Age 0 and Age 1 for Steelhead,  Pattern No. 4  No barrier for template.	c Upstream 3 highest 66 4 1 SSHEAR; HWG	3	12	185	9	61
