# Montana 5th-Code Watersheds

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: USDA Natural Resources Conservation Service
      Publication_Date: 19961112
      Title: Montana 5th-Code Watersheds
      Geospatial_Data_Presentation_Form: vector digital data
      Publication_Information:
        Publication_Place: Helena, Montana
        Publisher: Montana State Library
      Online_Linkage: \\FISH\VOL2\depts\gis\data\huc\mt\mt_huc
      Online_Linkage: \\FISH\VOL2\depts\gis\data\huc\mt\mt_huc
  Description:
    Abstract:
      This data set contains hydrologic unit boundaries at the Watershed (5th-Code) level. The data set was developed by delineating the boundary lines on 1:100,000 scale base maps or overlays and digitizing the delineated lines. 5th-code number assignment is subject to change in 4th-code units that span state boundaries as final 5th-code boundaries are developed for North Dakota, South Dakota, and Wyoming. The coverage version of this data set also has a region subclass named "fourcode" that contains the 4th-code sub-basins. For 4th-code sub-basins in shapefile format, see <http://nris.state.mt.us/nsdi/nris/subbasin.html>.
    Purpose:
      The watershed hydrologic unit boundary provides a uniquely identified and uniform method of subdividing large drainage areas. These smaller sized hydrologic units (approximately 40,000 to 250,000 acres) are useful in many programs supported by the Natural Resources Conservation Service and others.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 1996
    Currentness_Reference: publication date
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: Unknown
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -116.177956
      East_Bounding_Coordinate: -103.610898
      North_Bounding_Coordinate: 49.182360
      South_Bounding_Coordinate: 44.237954
    Data_Set_G-Polygon:
      Data_Set_G-Polygon_Outer_G-Ring:
        G-Ring:
          -116.0748825073,49.02441787719,-116.0513381958,47.93949127197,-115.7472457885,47.45859146118,-114.6641998291,46.60823059082,-114.424659729,46.61886978149,-114.5483016967,45.60388565063,-114.3186950683,45.43321228027,-113.9458312988,45.58434677124,-113.5072631835,44.86284637451,-112.8395233154,44.31266784668,-110.9373550415,44.44471740722,-110.950553894,44.95633697509,-108.1549987793,44.98777389526,-103.8922653198,44.98892211914,-103.7473602294,49.05199050903,-109.5802764892,49.08559036254,-116.0748825073,49.02441787719
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: Hydrologic unit
      Theme_Keyword: Watershed boundary
      Theme_Keyword: Drainage basin
    Place:
      Place_Keyword_Thesaurus: None
      Place_Keyword: Montana
  Access_Constraints: None
  Use_Constraints:
    The U.S. Department of Agriculture, Natural Resources Conservation Service, Montana State Office, should be acknowledged as the data source in products derived from these data.

    This data set is to be used as a primary reference source. This is public information and may be interpreted by organizations, agencies, units of government, or other based on needs, however, they are responsible for the appropriate application. Federal, State, or local regulatory bodies are not to reassign to the Natural Resources Conservation Service any authority for the decisions they make. Photographic or digital enlargement of this map to scales greater than 1:100,000 can cause misrepresentation of the data. If enlarged, the maps will not include the fine detail that would be appropriate for mapping at the large scale. Digital data files are periodically updated. Files are dated, and users are responsible for obtaining the latest revision of the data.

    Although these data have been processed successfully on a computer system at the U.S. Department of Agriculture, no warranty expressed or implied is made by the agency regarding the utility of the data on any other system, nor shall the act of distribution constitute any such warranty.

    The U.S. Department of Agriculture, nor any of its agencies are liable for misuse of the data. Nor is it liable for damage, transmission of viruses, or computer contamination through the distribution of these data sets.

  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Montana State Library
        Contact_Person: Gerry Daumiller
      Contact_Position: Senior GIS Programmer
      Contact_Address:
        Address_Type: mailing address
        Address: PO Box 201800
        City: Helena
        State_or_Province: Montana
        Postal_Code: 59620-1800
        Country: USA
      Contact_Voice_Telephone: (406) 444-5358
      Contact_Facsimile_Telephone: (406) 444-0581
      Contact_Electronic_Mail_Address: gdaumiller@state.mt.us
      Hours_of_Service: Monday-Friday, 8-5, Mountain Time
  Browse_Graphic:
    Browse_Graphic_File_Name: <http://nris.state.mt.us/nsdi/nris/hd109.gif>
    Browse_Graphic_File_Description: Simple image of the data set and/or its extent.
    Browse_Graphic_File_Type: GIF
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.0.0.535

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report:
      Polygon identifiers are manually checked with the original base map using the attribute file. Verification on polygon identification continuity of each side of a neatline is done visually on the computer screen as adjacent quad representations are assembled into larger area data layers.
  Logical_Consistency_Report:
    Certain node/geometry and topology polygon/chain relationships are collected or generated to satisfy topological requirements including: chains must begin and end at nodes and there are no duplicate lines or sliver polygons. Data beyond the state boundary is not included and is clipped at the boundary. All internal polygons are texted for closure and are checked using hard copy check plots. All data are checked for common boundary lines (i.e. adjacent polygons with the same label).
  Completeness_Report:
    The data is complete for the state of Montana. Meets national USDA NRCS specifications for the delineation of 5th-Code watersheds. Further delineation at the Sub-watershed (6th-code) level will be completed on an as-needed basis to meet USDA NRCS mission objectives. Sub-watersheds (10,000 to 40,000 acres) will be delineated using a base map scale of 1:24,000. The Subwatershed coverage will meet specifications as set forth in Natural Resources Conservation Service National Instruction 170-304 (revised).
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        The approximate horizontal accuracy of the base maps is 51 meters, assuming they meet National Map Accuracy Standards. The accuracy of the watershed maps is generally based on contour information available for the base maps. Such data may be supplemented with site visits to locate ridge lines for hydrologic unit boundaries in flat terrain areas or to identify changes in drainage patterns due to human or geologic activity. The difference in positional accuracy between the hydrologic unit boundaries and their digitized map locations is unknown.

        Hydrologic unit boundaries generally were digitized to be within 0.01 inches of their locations on the digitizing source (25 meters on the ground). The digital map elements are edge matched against the data for the adjacent quadrangle. Edge match locations generally do not deviate from centerline to centerline by more than 0.01 inches.

  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator:
            National Mapping Division U.S. Geological Survey
          Title: 1:100,000-scale quadrangles
          Geospatial_Data_Presentation_Form: map
          Publication_Information:
            Publication_Place: Reston, VA
            Publisher: U.S. Geological Survey
      Source_Scale_Denominator: 100000
      Type_of_Source_Media: stable based media or paper
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Range_of_Dates/Times:
            Beginning_Date: 1950
            Ending_Date: 1996
        Source_Currentness_Reference: publication date
      Source_Citation_Abbreviation: Q100
      Source_Contribution:
        These are the base maps upon which the watershed boundaries were drafted and digitized from.
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator:
            USDA Natural Resources Conservation Service Montana State Office
          Publication_Date: 1996
          Title: 5th-Code Watersheds
          Geospatial_Data_Presentation_Form: map
          Publication_Information:
            Publication_Place: Bozeman, Montana
            Publisher: USDA NRCS Montana State Office
      Source_Scale_Denominator: 100000
      Type_of_Source_Media: stable base media or paper
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 1996
        Source_Currentness_Reference: Publication Date
      Source_Citation_Abbreviation: scs1
      Source_Contribution: These are the watershed maps that were digitized.
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: U.S. Department of Agriculture
          Publication_Date: 19950601
          Title:
            Mapping and Digitizing Watershed and Subwatershed HUC Boundaries
          Geospatial_Data_Presentation_Form: other
          Publication_Information:
            Publication_Place: Washington, DC
            Publisher: Natural Resources Conservation Service
          Other_Citation_Details:
            NRCS National Instruction 170-304 Available at <http://www.nhq.nrcs.usda.gov/hu/intro.html>
      Type_of_Source_Media: text
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 19950601
        Source_Currentness_Reference: Publication Date
      Source_Citation_Abbreviation: hdgu
      Source_Contribution:
        These are the NRCS national guidelines for mapping and digitizing watersheds that were followed in preparation of this data set.
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: Idaho Department of Water Resources
          Publication_Date: 1996
          Title: Idaho 5th-Code Watersheds
          Geospatial_Data_Presentation_Form: map
          Publication_Information:
            Publication_Place: Boise, Idaho
            Publisher: Idaho Department of Water Resources
      Source_Scale_Denominator: 100000
      Type_of_Source_Media: electronic file
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 1996
        Source_Currentness_Reference: Publication Date
      Source_Citation_Abbreviation: idwr
      Source_Contribution:
        This is the source of the 5th-Code watershed boundaries in Idaho.
    Process_Step:
      Process_Description:
        Draft watershed boundaries on base maps based on the stream network and contours shown on the base maps and based on field investigations.
      Source_Used_Citation_Abbreviation: Q100
      Source_Used_Citation_Abbreviation: hdgu
      Process_Date: 1996
      Source_Produced_Citation_Abbreviation: scs1
    Process_Step:
      Process_Description:
        Digitize 1:100,000 scale hydrologic unit quadrangles in GRASS GIS.
      Source_Used_Citation_Abbreviation: scs1
      Source_Used_Citation_Abbreviation: hdgu
      Process_Date: 1996
      Source_Produced_Citation_Abbreviation: scs2
    Process_Step:
      Process_Description:
        Project quads from UTM zone 11 and 13 into zone 12 and match all the edges
      Source_Used_Citation_Abbreviation: scs2
      Process_Date: 1996
      Source_Produced_Citation_Abbreviation: scs3
    Process_Step:
      Process_Description: Verification of draft delineations by Montana NRCS field staff.
      Source_Used_Citation_Abbreviation: scs3
      Process_Date: 19960401
      Source_Produced_Citation_Abbreviation: scs4
    Process_Step:
      Process_Description:
        Verification of draft delineations by U.S. Forest Service Region One field staff.
      Source_Used_Citation_Abbreviation: scs4
      Process_Date: 19960901
      Source_Produced_Citation_Abbreviation: scs5
    Process_Step:
      Process_Description: Quality check digital data and hard copy plots.
      Source_Used_Citation_Abbreviation: scs5
      Process_Date: 19961001
      Source_Produced_Citation_Abbreviation: scs6
    Process_Step:
      Process_Description:
        Convert data from GRASS to Arc/Info format at Montana State Library.
      Source_Used_Citation_Abbreviation: scs6
      Process_Date: 19961003
      Source_Produced_Citation_Abbreviation: scs7
    Process_Step:
      Process_Description:
        Correct errors introduced by the Arc/Info conversion process. Project data to State Plane Coordinates and add complete boundaries of HUCs that cross the Idaho state line.
      Source_Used_Citation_Abbreviation: scs7
      Source_Used_Citation_Abbreviation: idwr
      Process_Date: 19961101
      Source_Produced_Citation_Abbreviation: scs8
    Process_Step:
      Process_Description:
        changed coding of lines and polys between 17010101090 and 17010102040 per faxed transmittal from NRCS Bozeman at request of FWP knowledge of watershed character.
      Process_Date: 19990614
    Process_Step:
      Process_Description: Metadata imported.
      Source_Used_Citation_Abbreviation: C:\DOCUME~1\cw8934\LOCALS~1\Temp\xml14.tmp

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: Complete chain
      Point_and_Vector_Object_Count: 4028
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: Label point
      Point_and_Vector_Object_Count: 889
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: GT-polygon composed of chains
      Point_and_Vector_Object_Count: 889
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: Point
      Point_and_Vector_Object_Count: 4
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: Composite object
      Point_and_Vector_Object_Count: 100

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: State Plane Coordinate System 1983
        State_Plane_Coordinate_System:
          SPCS_Zone_Identifier: 2500
          Lambert_Conformal_Conic:
            Standard_Parallel: 45.000000
            Standard_Parallel: 49.000000
            Longitude_of_Central_Meridian: -109.500000
            Latitude_of_Projection_Origin: 44.250000
            False_Easting: 600000.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.002048
          Ordinate_Resolution: 0.002048
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: mt_huc.aat
      Entity_Type_Definition: Arc Attribute Table
      Entity_Type_Definition_Source: ESRI
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: FNODE#
      Attribute_Definition: Internal node number for the beginning of an arc (from-node).
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: TNODE#
      Attribute_Definition: Internal node number for the end of an arc (to-node).
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: LPOLY#
      Attribute_Definition: Internal node number for the left polygon.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: RPOLY#
      Attribute_Definition: Internal node number for the right polygon.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: LENGTH
      Attribute_Definition: Length of feature in internal units.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: MT_HUC#
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: MT_HUC-ID
      Attribute_Definition: User-defined feature number.
      Attribute_Definition_Source: ESRI
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: mt_huc.pat
      Entity_Type_Definition: Polygon Attribute Table
      Entity_Type_Definition_Source: ESRI
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: AREA
      Attribute_Definition: Area of feature in internal units squared.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: PERIMETER
      Attribute_Definition: Perimeter of feature in internal units.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: MT_HUC#
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: MT_HUC-ID
      Attribute_Definition: User-defined feature number.
      Attribute_Definition_Source: ESRI
    Attribute:
      Attribute_Label: FIFTHCODE
      Attribute_Definition: 5th-Code watershed Hydrologic Unit Code (HUC) number
      Attribute_Definition_Source: NRCS
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 10010001010
          Range_Domain_Maximum: 17010213140
      Beginning_Date_of_Attribute_Values: 1996
    Attribute:
      Attribute_Label: FOURCODE
      Attribute_Definition: 4th-Code sub-basin Hydrologic Unit Code (HUC) number
      Attribute_Definition_Source: NRCS
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 10010001
          Range_Domain_Maximum: 17010213
      Beginning_Date_of_Attribute_Values: 1996
    Attribute:
      Attribute_Label: ACRES
      Attribute_Definition: Area of 5th-Code watershed in acres
      Attribute_Definition_Source: NRIS
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 1477
          Range_Domain_Maximum: 284938
      Beginning_Date_of_Attribute_Values: 1996
    Attribute:
      Attribute_Label: NAME
      Attribute_Definition:
        Name of the 4th-code sub-basin that contains this 5th-code watershed
      Attribute_Definition_Source: NRIS
      Attribute_Domain_Values:
        Unrepresentable_Domain: Character String
      Beginning_Date_of_Attribute_Values: 1996
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: mt_huc.patfourcode
      Entity_Type_Definition: Region Attribute Table
      Entity_Type_Definition_Source: ESRI
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: AREA
      Attribute_Definition: Area of feature in internal units squared.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: PERIMETER
      Attribute_Definition: Perimeter of feature in internal units.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: FOURCODE#
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: FOURCODE-ID
      Attribute_Definition: User-defined feature number.
      Attribute_Definition_Source: ESRI
    Attribute:
      Attribute_Label: FOURCODE
      Attribute_Definition: 4th-Code sub-basin Hydrologic Unit Code (HUC) number
      Attribute_Definition_Source: NRCS
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 10010001
          Range_Domain_Maximum: 17010213
      Beginning_Date_of_Attribute_Values: 1996
    Attribute:
      Attribute_Label: NAME
      Attribute_Definition: Name of the 4th-code sub-basin
      Attribute_Definition_Source: NRIS
      Attribute_Domain_Values:
        Unrepresentable_Domain: Character String
      Beginning_Date_of_Attribute_Values: 1996

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Montana State Library
        Contact_Person: Gerry Daumiller
      Contact_Position: Senior GIS Programmer
      Contact_Address:
        Address_Type: mailing address
        Address: PO Box 201800
        City: Helena
        State_or_Province: Montana
        Postal_Code: 59620-1800
        Country: USA
      Contact_Voice_Telephone: (406) 444-5358
      Contact_Facsimile_Telephone: (406) 444-0581
      Contact_Electronic_Mail_Address: gdaumiller@state.mt.us
      Hours_of_Service: Monday-Friday, 8-5, Mountain Time
  Resource_Description: Downloadable Data
  Distribution_Liability:
    Users must assume responsibility to determine the usability of this data for their purposes.
  Standard_Order_Process:
    Non-digital_Form:
      Contact the State Library to see if the data is available as hardcopy maps.
    Fees:
      For-profit organizations must pay our costs to reproduce the data. Fees can be waived if doing Government work.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: Arc/Info Export
        Transfer_Size: 8.198
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name: <http://nris.state.mt.us/nsdi/nris/e00/hd109.zip>
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ESRI Shapefile
        Transfer_Size: 8.198
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name: <http://nris.state.mt.us/nsdi/nris/shape/hd109.zip>
    Fees: None

Metadata_Reference_Information:
  Metadata_Date: 20050919
  Metadata_Review_Date: 19990616
  Metadata_Review_Date: 20030610
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Montana State Library
        Contact_Person: Gerry Daumiller
      Contact_Address:
        Address_Type: mailing address
        Address: PO Box 201800
        City: Helena
        State_or_Province: Montana
        Postal_Code: 59620-1800
        Country: USA
      Contact_Voice_Telephone: (406) 444-5358
      Contact_Facsimile_Telephone: (406) 444-0581
      Contact_Electronic_Mail_Address: gdaumiller@state.mt.us
      Hours_of_Service: Monday-Friday, 8-5, Mountain Time
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.8.6 on Mon Sep 19 16:15:08 2005