5	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	23	4	31
6	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	24	4	32
31	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	49	4	32
32	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	50	4	61
33	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	51	4	62
34	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	52	4	101
35	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	53	4	102
36	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	54	4	162
7	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	25	4	61
8	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	26	4	62
9	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	27	4	101
10	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	28	4	102
11	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	29	4	162
12	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	30	9	31
13	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	31	9	32
14	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	32	9	61
15	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	33	9	62
16	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	34	9	101
17	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	35	9	102
18	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	36	9	141
19	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	37	9	142
20	Kellogg Creek Fish Ladder				Aged fish ladder at the mouth of Kellogg Creek to the Willamette River; structure also works as a dam, and creates Kellogg Lake at the mouth as well.  ODOT has retrofitted the ladder and it is no longer a barrier to fish.	This fish ladder worked only for the strongest adults (steelhead, coho, chinook); during low flow and high flow, the ladder was a barrier.  ODOT has retrofitted the ladder.		936	38	9	162
21	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	39	9	31
22	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	40	9	32
23	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	41	9	61
24	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	42	9	62
25	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	43	9	101
26	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	44	9	102
27	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	45	9	141
28	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	46	9	142
29	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	47	9	162
30	Headwall				Headwall constructed in Cedar Creek for inline stormwater detention; does not work ever for stormwater detention.	Cement headwall constructed in stream channel to back water up behind it for stormwater detention; this design does not work.  Issues are high jump (12"+) and velocity issues through the "slot".	2	944	48	4	31
