# flow_station

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator:
        Original station location descriptions and/or Latitude and Longitude information came from the USGS. Data were compiled and translated into this point shapefile by the Technical Outreach and Assistance Team (TOAST; sponsored by the Columbia River Inter-Tribal Fish Commission).
      Publication_Date:
        REQUIRED: The date when the data set is published or otherwise made available for release.
      Publication_Time: Oct 30, 2004
      Title: flow_station
      Edition: Draft-1
      Geospatial_Data_Presentation_Form: vector digital data
      Other_Citation_Details:
        Some corrections were made to USGS station locations by the author (using Terrain Navigator Software) in coordination with Oregon based USGS staff. All locations are an approximation. Please check with original sources of data for exact locations.
      Online_Linkage:
        \\Fish\vol2\Depts\GIS\project\subbasin_planning\archive\gis_data\umatilla_willow\willow\flow_station.shp
  Description:
    Abstract:
      This DRAFT spatial dataset includes point flow stations and descriptions based primarily on data from the US Geological Survey (USGS) for Oregon daily flow. Each point represents a location where data for daily flow were gathered, analyzed, and associated with a stream reach for purposes of modeling fish habitat.
    Purpose:
      The flow stations represented here are locations where flow data were gathered, analyzed and presented to each Oregon subbasin team for their work with Mobrand Biometric's Ecosystem Diagnostic and Treatment (EDT; <http://www.mobrand.com/MBI/edt.html>) model during the 2002-2004 Oregon Subbasin Planning effort.
    Supplemental_Information:
      The flow data gathered and analyzed for each of these stations are located in Access databases built for each Oregon subbasin team for the 2002-2004 Subbasin Planning effort. The databases are archived with StreamNet.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2003
    Currentness_Reference: ground condition - check dates that data were collected
  Status:
    Progress: In work- Draft
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -120.014934
      East_Bounding_Coordinate: -119.428257
      North_Bounding_Coordinate: 45.754565
      South_Bounding_Coordinate: 45.257593
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus:
        REQUIRED: Reference to a formally registered thesaurus or a similar authoritative source of theme keywords.
      Theme_Keyword: flow station
  Access_Constraints:
    None: these are public data gathered from public sources (USGS).
  Use_Constraints:
    While these data were available from public sources, corrections have been made to rectify latitude and longitude errors that located points away from the station location descriptions. Through communication with the USGS, some stations were relocated to the correct position (using Terrain Navigator Software) and may no longer match the original latitude and longitude information found at the USGS website: <http://nwis.waterdata.usgs.gov/or/nwis/discharge/?search_criteria=search_site_no&submitted_form=introduction> All station points are in the approximate physical location of the stations.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Denise Kelsey
        Contact_Organization: Columbia River Inter-Tribal Fish Commission
      Contact_Position: Fishery Biologist
      Contact_Voice_Telephone: 503-731-1280
      Contact_Facsimile_Telephone: 503-235-4228
      Contact_Electronic_Mail_Address: keld@critfc.org
      Hours_of_Service: M-F 8AM - 4PM
      Contact_Instructions:
        Contact Denise for information regarding station placement information or check the USGS website at <http://nwis.waterdata.usgs.gov/or/nwis/discharge/?search_criteria=search_site_no&submitted_form=introduction>
  Native_Data_Set_Environment:
    Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 4; ESRI ArcCatalog 8.3.0.800

Data_Quality_Information:
  Lineage:
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation:
        C:\Documents and Settings\keld.DENISE\My Documents\GIS Requests\work\umatilla\willow\flow_station

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: Entity point
      Point_and_Vector_Object_Count: 6

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Map_Projection:
        Map_Projection_Name: Lambert Conformal Conic
        Lambert_Conformal_Conic:
          Standard_Parallel: 43.000000
          Standard_Parallel: 45.500000
          Longitude_of_Central_Meridian: -120.500000
          Latitude_of_Projection_Origin: 41.750000
          False_Easting: 1312336.000000
          False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.000256
          Ordinate_Resolution: 0.000256
        Planar_Distance_Units: User_Defined_Unit
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: flow_station
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: RECORD
      Attribute_Definition: Whole unique numbers assigned.
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: SUBBASIN
      Attribute_Definition: Columbia River subbasin where station is located.
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: AGENCY
      Attribute_Definition: Source of station information and data.
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: SITE_NO
      Attribute_Definition: Site number; unique station code.
      Attribute_Definition_Source: USGS
    Attribute:
      Attribute_Label: STATION_NM
      Attribute_Definition: Description of physical station location.
      Attribute_Definition_Source: USGS
    Attribute:
      Attribute_Label: DEC_LAT
      Attribute_Definition: datum code for decimal latitude.
      Attribute_Definition_Source: USGS website or Terrain Navigator mapping program
    Attribute:
      Attribute_Label: DEC_LONG
      Attribute_Definition: datum code for decimal longitude.
      Attribute_Definition_Source: USGS website or Terrain Navigator mapping program
    Attribute:
      Attribute_Label: DATUM_CD
      Attribute_Definition: Number for USGS Fourthfield Hydrological Unit (HUC)
      Attribute_Definition_Source: USGS
    Attribute:
      Attribute_Label: FROM_
      Attribute_Definition: First year flow data were reported.
      Attribute_Definition_Source: USGS
    Attribute:
      Attribute_Label: TO
      Attribute_Definition: Last year flow data were reported.
      Attribute_Definition_Source: USGS
    Attribute:
      Attribute_Label: REACH_NM
      Attribute_Definition:
        EDT modeling code for stream reaches associated with the flow station.
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: STREAM_NM
      Attribute_Definition:
        Stream name assigned by StreamNet or found on the USGS 1:24,000 digital raster graphic (DRG) images
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: COMMENTS
      Attribute_Definition:
        Additional information regarding station location or data reported by the station
      Attribute_Definition_Source: TOAST

Distribution_Information:
  Resource_Description: Downloadable Data
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 0.018

Metadata_Reference_Information:
  Metadata_Date: 20041026
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Columbia River Inter-Tribal Fish Commission
        Contact_Person: Denise Kelsey
      Contact_Position: Fishery Biologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 729 NE Oregon Street, Suite 200
        City: Portland
        State_or_Province: OR
        Postal_Code: 97232
        Country: USA
      Contact_Voice_Telephone: 503-731-1280
      Contact_Facsimile_Telephone: 503-235-4228
      Contact_Electronic_Mail_Address: keld@critfc.org
      Hours_of_Service: M-F 8AM - 4PM
      Contact_Instructions:
        Metadata were created by Denise Kelsey and Jennifer Brainard. Contact Denise regarding metadata and stations.
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.7.33 on Tue Oct 26 11:02:31 2004