# wq_station

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator:
        Original station location descriptions and/or Latitude and Longitude information came from the ODEQ staff. Data were compiled and translated into this point shapefile by the Technical Outreach and Assistance Team (TOAST; sponsored by the Columbia River Inter-Tribal Fish Commission).
      Publication_Date: August 1, 2004
      Publication_Time: noon
      Title: wq_station
      Edition: Draft-1
      Geospatial_Data_Presentation_Form: vector digital data
      Other_Citation_Details:
        Some corrections were made to ODEQ station locations by the author in coordination with Oregon based DEQ staff. Stations identified from other sources were located by physical description only, therefore errors in placement could have occurred. All locations are an approximation. Please check with original sources of data for exact locations.
      Online_Linkage: none currently--data available on request
  Description:
    Abstract:
      This DRAFT spatial dataset includes point (continuous temperature and water quality grab sample) stations and descriptions based on data from the Oregon Department of Enviromental Quality (ODEQ) laser database or sent directly to us by ODEQ staff. Each point represents a location where data were gathered, analyzed, and associated with a stream reach for purposes of modeling fish habitat.
    Purpose:
      The ODEQ stations represented here are locations where data were gathered, analyzed, and presented to each Oregon subbasin team for their work with Mobrand Biometric's Ecosystem Diagnostic and Treatment (EDT; <http://www.mobrand.com/MBI/edt.html>) model during the 2002-2004 Oregon Subbasin Planning effort.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2003
    Currentness_Reference: ground condition - check dates that data were collected
  Status:
    Progress: In work / DRAFT
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -117.734374
      East_Bounding_Coordinate: -117.225631
      North_Bounding_Coordinate: 44.580077
      South_Bounding_Coordinate: 44.356451
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus:
        REQUIRED: Reference to a formally registered thesaurus or a similar authoritative source of theme keywords.
      Theme_Keyword: water quality, station, temperature
  Access_Constraints:
    None: these are public data gathered from public sources (ODEQ).
  Use_Constraints:
    While these data were available from public sources, corrections have been made to rectify latitude and longitude errors that located points away from the station location descriptions. Through communication with the ODEQ, some stations were relocated to the correct position and may no longer match the original latitude and longitude information found at the ODEQ website: <http://www.deq.state.or.us/wq/> All station points are in the approximate physical location of the stations.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Denise Kelsey
        Contact_Organization: Columbia River Inter-Tribal Fish Commission
      Contact_Position: Fishery Biologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 729 NE Oregon Street, Suite 200
        City: Portland
        State_or_Province: OR
        Postal_Code: 97232
        Country: USA
      Contact_Voice_Telephone: 503-731-1280
      Contact_Facsimile_Telephone: 503-235-4228
      Contact_Electronic_Mail_Address: keld@critfc.org
      Hours_of_Service: M-F 8AM - 4PM
      Contact_Instructions:
        Metadata were created by Denise Kelsey and Jennifer Brainard. Contact Denise regarding metadata and WQ and Temperature stations.
  Data_Set_Credit:
    ODEQ data from the laser database were obtained from directly from ODEQ by request. Other data were submitted by Oregon Department of Environmental Quality (ODEQ; Bonnie Lamb) from the Barlow Ranger District.
  Native_Data_Set_Environment:
    Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 4; ESRI ArcCatalog 8.3.0.800

Data_Quality_Information:
  Lineage:
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation: C:\gis\work\flow\deq_station
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation:
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation: C:\gis\work\flow\wq_station
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation: C:\gis\work\flow_wq\wq_station
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation: \\Fish\vol2\Depts\GIS\data\hydro\or\wq_station
    Process_Step:
      Process_Description: Dataset copied.
      Source_Used_Citation_Abbreviation:

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: Entity point
      Point_and_Vector_Object_Count: 12

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Map_Projection:
        Map_Projection_Name: Lambert Conformal Conic
        Lambert_Conformal_Conic:
          Standard_Parallel: 43.000000
          Standard_Parallel: 45.500000
          Longitude_of_Central_Meridian: -120.500000
          Latitude_of_Projection_Origin: 41.750000
          False_Easting: 1312336.000000
          False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.000256
          Ordinate_Resolution: 0.000256
        Planar_Distance_Units: User_Defined_Unit
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: wq_station
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: AREA
    Attribute:
      Attribute_Label: PERIMETER
    Attribute:
      Attribute_Label: RECORD
      Attribute_Definition: Unique number identifier for each station.
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: SUBBASIN
      Attribute_Definition:
        The name of the Columbia River Subbasin in which the stations is located.
      Attribute_Definition_Source: ODEQ
    Attribute:
      Attribute_Label: STATION_NO
      Attribute_Definition: Agency code for station identification
      Attribute_Definition_Source: ODEQ, USFS, ODFW, SWCD, HRWG, MFID, CTWS
    Attribute:
      Attribute_Label: LOCATION
      Attribute_Definition: Description of physical station location
      Attribute_Definition_Source: ODEQ, USFS, ODFW, SWCD, HRWG, MFID, CTWS
    Attribute:
      Attribute_Label: DEC_LONG
      Attribute_Definition: station location longitude in decimal degrees
      Attribute_Definition_Source: ODEQ or Terrain Navigator mapping program
    Attribute:
      Attribute_Label: DEC_LAT
      Attribute_Definition: station location latitude in decimal degrees
      Attribute_Definition_Source: ODEQ or Terrain Navigator mapping program
    Attribute:
      Attribute_Label: AGENCY
      Attribute_Definition: agency source of data
      Attribute_Definition_Source: ODEQ, USFS, ODFW, SWCD, HRWG, MFID, CTWS
    Attribute:
      Attribute_Label: SOURCE
      Attribute_Definition: agency with which the data originated
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: SOURCE_CD
      Attribute_Definition:
        code from source agency for station identification, some stations will also have a ODEQ laser database code located in Station_No
      Attribute_Definition_Source: ODEQ, USFS, ODFW, SWCD, HRWG, MFID, CTWS
    Attribute:
      Attribute_Label: DATA_TYPE
      Attribute_Definition:
        WQ - grab samples for water quality, Temp - continuous temperature
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: REACH_NAME
      Attribute_Definition:
        EDT modeling code for stream reaches associated with the station
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: FEAT_NAME
      Attribute_Definition:
        Stream name assigned by StreamNet or found on the USGS 1:24,000 digital raster graphic (DRG) images
      Attribute_Definition_Source: TOAST
    Attribute:
      Attribute_Label: COMMENT
      Attribute_Definition:
        Additional information regarding station location or data reported by the station
      Attribute_Definition_Source: TOAST

Distribution_Information:
  Resource_Description: Downloadable Data
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 0.132

Metadata_Reference_Information:
  Metadata_Date: 20041014
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Columbia River Inter-Tribal Fish Commission
        Contact_Person: Denise Kelsey
      Contact_Position: Fishery Biologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 729 NE Oregon Street, Suite 200
        City: Portland
        State_or_Province: OR
        Postal_Code: REQUI97232
        Country: USA
      Contact_Voice_Telephone: 503-731-1280
      Contact_Facsimile_Telephone: 503-235-4228
      Contact_Electronic_Mail_Address: keld@critfc.org
      Hours_of_Service: M-F 8AM - 4PM
      Contact_Instructions:
        Metadata were created by Denise Kelsey and Jennifer Brainard. Contact Denise regarding metadata and stations.
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.7.33 on Thu Oct 14 11:55:53 2004